GSIC - Global Service Information Center

### DTC C0226/21 SFR Solenoid Circuit

### DTC C0236/22 SFL Solenoid Circuit

### DTC C0246/23 SRR Solenoid Circuit

## for Preparation Click here

## DESCRIPTION

ABS solenoids turn on when receiving signals from the ECU. They control braking force by adjusting the pressure applied to the wheel cylinders.

DTC No. | DTC Detection Condition | Trouble Area

C0226/21

Open or short circuit in front right solenoid circuit (SFRR or SFRH) continues for 0.05 sec. or more

1. SFRR or SFRH circuit
2. Brake actuator assembly

C0236/22

Open or short circuit in front right solenoid circuit (SFLR or SFLH) continues for 0.05 sec. or more

1. SFLR or SFLH circuit
2. Brake actuator assembly

C0246/23

Open or short circuit in front right solenoid circuit (SRRR or SRRH) continues for 0.05 sec. or more

1. SRRR or SRRH circuit
2. Brake actuator assembly

## WIRING DIAGRAM

## INSPECTION PROCEDURE

1.RECONFIRM DTC

HINT:

  These codes are output when a problem is detected in the brake actuator assembly.

  As the solenoid circuit is built into the brake actuator assembly, solenoid circuit inspection and solenoid unit inspection cannot be performed.

  Be sure to check if the DTC is output before replacing the brake actuator assembly.

1. Clear the DTCs.

1. Turn the ignition switch ON and check that the ABS warning light illuminates for approximately 3 seconds.

1. Check for DTCs.

   Result
   Result | Proceed to
   DTC is not output | A
   DTC is output | B

| B |

REPLACE BRAKE ACTUATOR ASSEMBLY

A |

2.PERFORM ACTIVE TEST BY INTELLIGENT TESTER (ABS SOLENOID)

1. Using the intelligent tester's Active Test, generate a control command and then check that the ABS solenoid operates.

   Skid control ECU
   Item | Vehicle Condition / Test Details | Diagnostic Note
   ABS Solenoid (SRRR) | Turns ABS solenoid (SRRR) ON / OFF | Operation of solenoid (clicking sound) can be heard
   ABS Solenoid (SRRH) | Turns ABS solenoid (SRRH) ON / OFF | Operation of solenoid (clicking sound) can be heard
   ABS Solenoid (SFLR) | Turns ABS solenoid (SFLR) ON / OFF | Operation of solenoid (clicking sound) can be heard
   ABS Solenoid (SFLH) | Turns ABS solenoid (SFLH) ON / OFF | Operation of solenoid (clicking sound) can be heard
   ABS Solenoid (SFRR) | Turns ABS solenoid (SFRR) ON / OFF | Operation of solenoid (clicking sound) can be heard
   ABS Solenoid (SFRH) | Turns ABS solenoid (SFRH) ON / OFF | Operation of solenoid (clicking sound) can be heard

| NG |

REPLACE BRAKE ACTUATOR ASSEMBLY

OK |

END