GSIC - Global Service Information Center

# OUTSIDE MOULDING > INSTALLATION

## for Preparation Click here

1. INSTALL NO. 1 REAR WHEEL OPENING EXTENSION LH

1. Attach the 11 clips to install the extension.

1. Install the 7 screws.

2. INSTALL NO. 1 REAR WHEEL OPENING EXTENSION RH

1. Attach the 12 clips to install the extension.

1. Install the 7 screws.

3. INSTALL FRONT WHEEL OPENING EXTENSION SUB-ASSEMBLY LH

1. Attach the 8 clips to install the extension.

1. Install the 7 screws.

4. INSTALL FRONT WHEEL OPENING EXTENSION SUB-ASSEMBLY RH

HINT:

  Use the same procedures described for the LH side.