GSIC - Global Service Information Center

# 2KD-FTV ENGINE CONTROL SYSTEM > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Diesel throttle body assembly x Intake air connector | 20 | 204 | 15
Engine cover sub-assembly x Charge air cooler assembly with intake air connector | 7.0 | 71 | 62 in.*lbf
ECM bracket No. 1 x ECM | 3.0 | 31 | 27 in.*lbf
ECM bracket No. 2 x ECM | 3.0 | 31 | 27 in.*lbf
ECM bracket No. 1 x Reinforcement | 12.5 | 128 | 9
ECM bracket No. 2 x Body | 12.5 | 128 | 9
Accelerator pedal rod assembly x Body | 5.0 | 51 | 44 in.*lbf