GSIC - Global Service Information Center

# 1GR-FE FUEL > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Fuel pressure regulator assembly x SST (Union) | 7.5 | 80 | 66 in.*lbf
Fuel delivery pipe sub-assembly x Intake manifold | 15 | 153 | 11
Intake air surge tank x Intake manifold | 28 | 286 | 21
Intake air surge tank x Throttle body bracket | 21 | 214 | 16
Intake air surge tank x No. 1 surge tank stay | 21 | 214 | 16
Throttle body bracket x Oil baffle plate | 9.0 | 92 | 80 in.*lbf
Intake air surge tank x No. 2 surge tank stay | 21 | 214 | 16
Fuel pressure regulator assembly x Fuel delivery pipe sub-assembly | 9.0 | 92 | 80 in.*lbf
Fuel filter assembly x Body | 8.5 | 87 | 75 in.*lbf
Fuel tank x Body | 61 | 622 | 45
No. 1 fuel tank protector sub-assembly x Body | 20 | 204 | 15
Fuel tank filler pipe sub-assembly x Body | 19 | 194 | 14