GSIC - Global Service Information Center

### REAR LEAF SPRING (for 2WD) > INSTALLATION

1. INSTALL REAR LH LEAF SPRING ASSEMBLY

2. INSTALL NO. 2 REAR LEAF SPRING SHACKLE SUB-ASSEMBLY

3. TEMPORARILY INSTALL LEAF SPRING SHACKLE INNER PLATE

4. TEMPORARILY INSTALL REAR LEAF SPRING BRACKET PIN OR PIN BOLT

5. TEMPORARILY TIGHTEN REAR LEAF SPRING U BOLT

6. INSTALL REAR LEAF SPRING BUMPER

7. INSTALL REAR SHOCK ABSORBER ASSEMBLY

8. INSTALL NO. 3 PARKING BRAKE CABLE

9. STABILIZE SUSPENSION

10. TIGHTEN LEAF SPRING SHACKLE INNER PLATE NUT

11. TIGHTEN REAR LEAF SPRING BRACKET PIN NUT

12. TIGHTEN REAR LEAF SPRING PIN SET BOLT

13. TIGHTEN LEAF SPRING U BOLT SEAT NUT

14. INSTALL REAR WHEEL