GSIC - Global Service Information Center

### VANE PUMP (for KD Series Engine) > INSTALLATION

1. INSTALL VANE PUMP ASSEMBLY

2. CONNECT PRESSURE FEED TUBE ASSEMBLY

3. CONNECT OIL RESERVOIR TO PUMP HOSE

4. ADD POWER STEERING FLUID

5. BLEED AIR FROM POWER STEERING SYSTEM

6. CHECK POWER STEERING FLUID LEVEL IN RESERVOIR

7. INSPECT FOR FLUID LEAKS

8. INSTALL FRONT SIDEMEMBER TO FRONT SUSPENSION CROSSMEMBER BRACE

9. INSTALL NO. 1 ENGINE UNDER COVER (for 4WD)

10. INSTALL NO. 2 ENGINE UNDER COVER (for 4WD)