GSIC - Global Service Information Center

# BLOWER UNIT > REASSEMBLY

## for Preparation Click here

1. INSTALL BLOWER W/FAN MOTOR SUB-ASSEMBLY

1. Install the blower motor with the 3 screws.

2. INSTALL BLOWER RESISTOR

1. Install the blower resistor with the 2 screws.

3. INSTALL AIR INLET DAMPER CONTROL CABLE SUB-ASSEMBLY

1. Attach the 3 claws to install the cable.

4. INSTALL NO. 3 AIR DUCT

1. Attach the 4 claws to install the duct.