GSIC - Global Service Information Center

# PARK / NEUTRAL POSITION SWITCH > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT PARK/NEUTRAL POSITION SWITCH ASSEMBLY

1. Apply the parking brake and turn the ignition switch ON.

1. Depress the brake pedal and check that the engine starts when the shift lever is on N or P, but does not start in other positions.

1. Check that the back-up lamp illuminates and the reverse warning buzzer sounds when the shift lever is on R, but do not function in other positions.