GSIC - Global Service Information Center

# BRAKE > TORQUE SPECIFICATIONS

Brake fluid:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Brake line x Brake master cylinder sub-assembly (without SST) | 15.2 | 155 | 11
  Brake line x Brake master cylinder sub-assembly (with SST) | 14 | 143 | 10
  Front disc brake bleeder plug (2WD) | 10.8 | 110 | 8
  Rear bleeder plug (2WD) | 11 | 112 | 8
  Rear bleeder plug (4WD) | 10 | 102 | 7

Brake pedal:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Push rod clevis lock nut | 26 | 265 | 19
  Brake pedal shaft | 37 | 377 | 27
  Stop light switch x Stop light switch mounting adjuster | 1.5 | 15 | 13 in.*lbf
  Brake pedal support sub-assembly x Brake booster assembly | 14.2 | 145 | 10
  Brake pedal support sub-assembly x Instrument panel reinforcement | 21 | 214 | 15

Brake master cylinder:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Brake master cylinder sub-assembly x Brake booster | 20 | 204 | 15
  Brake line x Brake master cylinder sub-assembly (without SST) | 15.2 | 155 | 11
  Brake line x Brake master cylinder sub-assembly (with SST) | 14 | 143 | 10

Brake booster:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Brake booster assembly x Brae pedal support sub-assembly | 14.2 | 145 | 10
  Vacuum warning switch x Brae booster assembly | 13.7 | 139 | 10

Vacuum pump:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Gear lock nut | 110 | 1,122 | 81
  Vacuum pump end cover x Vacuum pump housing | 7.8 | 80 | 69 in.*lbf
  Check valve sub-assembly x Vacuum pump end cover | 74 | 755 | 54
  Union bolt x Union | 14 | 143 | 10
  Vacuum pump assembly | 21 | 214 | 15

Front brake (for 2WD):

  Part tightened | N*m | kgf*cm | ft.*lbf
  Front disc brake cylinder mounting x Steering knuckle | 117 | 1,193 | 86
  Disc brake cylinder assembly x Steering knuckle | 39.2 | 400 | 29
  Union bolt x Disc brake cylinder assembly | 29 | 296 | 21
  Front wheel (for steel type) | 152 | 1,550 | 112
  Front wheel (for aluminum type) | 121 | 1,234 | 89
  Front disc brake bleeder plug x Disc brake cylinder assembly | 10.8 | 110 | 8

Front brake (for4WD):

  Part tightened | N*m | kgf*cm | ft.*lbf
  Disc brake cylinder assembly x Steering knuckle | 122 | 1,244 | 90
  Front No. 1 wheel cylinder tube x Disc brake cylinder assembly (without SST) | 15.2 | 155 | 11
  Front No. 1 wheel cylinder tube x Disc brake cylinder assembly (with SST) | 14 | 143 | 10
  Front wheel | 105 | 1,071 | 77
  Front disc brake bleeder plug x Disc brake cylinder assembly | 10.8 | 110 | 8

Front brake flexible hose:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Union bolt x Disc brake cylinder assembly (2WD) | 29 | 296 | 21
  Front No. 1 wheel cylinder tube x Brake tube (2WD, without SST) | 15.2 | 155 | 11
  Front No. 1 wheel cylinder tube x Brake tube (2WD, with SST) | 14 | 143 | 10
  Front No. 1 wheel cylinder tube x Disc brake cylinder assembly (4WD, without SST) | 15.2 | 155 | 11
  Front No. 1 wheel cylinder tube x Disc brake cylinder assembly (4WD, with SST) | 14 | 143 | 10
  Front No. 1 wheel cylinder tube x Brake tube (4WD, without SST) | 15.2 | 155 | 11
  Front No. 1 wheel cylinder tube x Brake tube (4WD, with SST) | 14 | 143 | 10

Rear brake (for 2WD):

  Part tightened | N*m | kgf*cm | ft.*lbf
  Rear wheel brake cylinder assembly x Backing plate | 9.5 | 97 | 84in.*lbf
  Brake tube x Rear wheel brake cylinder assembly (without SST) | 15.2 | 155 | 11
  Brake tube x Rear wheel brake cylinder assembly (with SST) | 14 | 143 | 10
  Rear wheel (for steel type) | 152 | 1,550 | 112
  Rear wheel (for aluminum type) | 121 | 1,234 | 89
  Rear brake drum bleeder plug x Rear wheel brake cylinder assembly) | 11 | 112 | 8

Rear brake (for 4WD):

  Part tightened | N*m | kgf*cm | ft.*lbf
  Rear wheel brake cylinder assembly x Backing plate | 11.5 | 117 | 8
  Rear wheel brake cylinder assembly x Backing plate | 15.2 | 155 | 11
  Brake tube x Rear wheel brake cylinder assembly (with SST) | 14 | 143 | 10
  Rear wheel | 105 | 1,070 | 77
  Rear brake drum bleeder plug x Rear wheel brake cylinder assembly) | 10 | 102 | 7

Rear brake flexible hose:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Rear brake tube flexible hose x brake tube (without SST) | 15.2 | 155 | 11
  Rear brake tube flexible hose x brake tube (with SST) | 14 | 143 | 10
  Rear brake tube flexible hose x 3-way (without SST) | 15.2 | 155 | 11
  Rear brake tube flexible hose x 3-way (with SST) | 14 | 143 | 10

Load sensing proportioning valve:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Lock nut | 12.5 | 127 | 9
  Rear flexible hose bracket x valve body | 12.5 | 127 | 9
  Load sensing proportioning valve assembly x | 29.4 | 300 | 22
  Brake tube x Valve body (without SST) | 15.2 | 155 | 11
  Brake tube x Valve body (with SST) | 14 | 143 | 10
  No. 2 shackle x Rear differential | 29.4 | 300 | 22
  Lock nut | 12.5 | 127 | 9