GSIC - Global Service Information Center

# FRONT WIPER RUBBER > INSTALLATION

## for Preparation Click here

1. INSTALL WIPER RUBBER

1. Install the 2 packing plates to the rubber.

   NOTICE:
     Install the packing plates facing the proper direction.

1. Install the wiper rubber to the claw of the wiper blade in the direction indicated by the arrow in the illustration.

   HINT:
     Install the wiper rubber so that the head part (large side) of the wiper rubber faces the arm axle side.

1. Attach the head part (large side) of the wiper rubber to the rear end side claw of the wiper blade.

   NOTICE:
     Push the wiper blade into the grooves of the wiper rubber to attach them completely.

2. INSTALL FRONT WIPER BLADE

1. Attach the claw to install the wiper blade.