GSIC - Global Service Information Center

### OIL PUMP > DISASSEMBLY

1. REMOVE FRONT OIL PUMP BODY O-RING

2. FIX OIL PUMP ASSEMBLY

3. REMOVE CLUTCH DRUM OIL SEAL RING

4. REMOVE STATOR SHAFT THRUST BEARING RACE

5. REMOVE STATOR SHAFT ASSEMBLY

6. INSPECT FRONT OIL PUMP BODY

7. INSPECT STATOR SHAFT ASSEMBLY

8. INSPECT CLEARANCE OF FRONT OIL PUMP BODY

9. REMOVE FRONT OIL PUMP DRIVE GEAR

10. REMOVE FRONT OIL PUMP DRIVEN GEAR

11. REMOVE FRONT OIL PUMP OIL SEAL