GSIC - Global Service Information Center

### REAR SEAT OUTER BELT ASSEMBLY > INSTALLATION

1. INSTALL REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH

2. INSTALL QUARTER TRIM PANEL LOWER LH (for Double Cab)

3. INSTALL REAR DOOR OPENING TRIM LH (for Double Cab)

4. INSTALL REAR DOOR SCUFF PLATE LH (for Double Cab)

5. INSTALL REAR SEAT ASSEMBLY (for Extra Cab)

6. INSTALL QUARTER INSIDE TRIM BOARD LH (for Extra Cab)

7. INSTALL REAR SEAT CUSHION ASSEMBLY RH (for Extra Cab)

8. INSTALL REAR SEAT CUSHION ASSEMBLY LH (for Extra Cab)

9. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

10. PERFORM INITIALIZATION