GSIC - Global Service Information Center

# CLUTCH > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Clutch pedal sub-assembly x Clutch pedal support | 37 | 377 | 27
Clutch pedal support x Clutch master cylinder | 12 | 122 | 9
Clutch pedal support x Instrument panel reinforcement | 24 | 245 | 18
Cylinder push rod clevis lock nut | 12 | 122 | 9
Pedal height adjust nut | 25 | 255 | 18
Clutch master cylinder assembly x Clutch master cylinder to flexible hose | For use without SST | 15 | 153 | 11
For use with SST | 14 | 143 | 10
Release cylinder bleeder plug | 11 | 112 | 8
Clutch release cylinder x Manual transmission unit assembly | 1KD-FTV, 2KD-FTV, 2TR-FE | 12 | 122 | 9
Clutch release cylinder x Manual transmission unit assembly | 1GR-FE | 19 | 194 | 14
Release cylinder heat insulator x Clutch release cylinder | 1GR-FE | 12 | 120 | 9
Clutch release cylinder assembly x Clutch release cylinder flexible tube | For use without SST | 15 | 153 | 11
For use with SST | 14 | 143 | 10
Clutch cover assembly x Flywheel | 19 | 195 | 14
Clutch accumulator x Body | 18 | 184 | 13
Clutch accumulator x Flexible hose tube | For use without SST | 15 | 153 | 11
For use with SST | 14 | 143 | 10