GSIC - Global Service Information Center

MANUAL TRANSMISSION UNIT > REMOVAL > Preparation |

SST
| 09308-00010 | Oil Seal Puller
| 09817-16011 | Back-up Light Switch Tool
| 09950-40011 | Puller B Set
| (09951-04010) | Hanger 150
| (09952-04010) | Slide Arm
| (09953-04020) | Center Bolt 150
| (09954-04010) | Arm 25
| (09955-04011) | Claw No.1
| (09955-04051) | Claw No.5
| (09957-04010) | Attachment
| (09958-04011) | Holder
| 09950-50013 | Puller C Set
| (09951-05010) | Hanger 150
| (09952-05010) | Slide Arm
| (09953-05020) | Center Bolt 150
| (09954-05021) | Claw No.2
| (09957-04010) | Attachment

EQUIPMENT
Cylinder gauge | -
Dial indicator or dial indicator with magnetic base | -
Feeler gauge | -
Micrometer | -
Plastic hammer | -
Press | -
Torque wrench | -
Vernier calipers | -

LUBRICANT
Item | Capacity | Classification
Manual transmission oil | 2.2 liters (2.3 US qts, 1.9 lmp. qts) | API GL-4 or GL-5 SAE 75W-90

RECOMMENDED TOOLS
| 09031-00040 | Pin Punch . | -
| 09042-00020 | Torx Socket T40 | -
| 09905-00012 | Snap Ring No.1 Expander | -

SSM
| 08826-00090 | Seal Packing 1281, THREE BOND 1281 or equivalent (FIPG) | -