GSIC - Global Service Information Center

EXTENSION HOUSING REAR OIL SEAL > REMOVAL > Preparation |

SST
| 09308-00010 | Oil Seal Puller

EQUIPMENT
Feeler gauge |
Cylinder gauge |
Vernier calipers |
Dial indicator |
Micrometer |
Straight edge |
Torque wrench |
Angle gauge |
V block |
Dial indicator or dial indicator with magnetic base |

LUBRICANT
Automatic transmission fluid: Dry fill | 7.2 litter (7.61 US qts, 6.34 lmp.qts) | ATF WS
Automatic transmission fluid: Drain and refill | 1.7 litter (1.8 US qts, 1.5 lmp.qts) | ATF WS

RECOMMENDED TOOLS
| 09040-00011 | Hexagon Wrench Set | -
| (09043-20100) | Socket Hexagon Wrench 10 | -
| 09070-20010 | Moulding Remover | -
| (09043-20060) | Socket Hexagon Wrench 6 | -